For use:

1 ==> Put ON controller DATEC
2 ==> Plug cable between PC and DATEC.


3 ==> Launch software: FITASC_JPB.exe
4 ==> Wait cursor finish
      You must see one ligne with number of your DATEC
      
      ===> IF NOT: close software and launch another time 
                   without restart your DATEC.
      
      
5 ==> Click on START BOOTLOADER.
  ==> Say YES on all questions for update memory.
  
6 ==> Select the file for updating and click on OK

7 ==> Wait the end window.
8 ==> click on OK for close

End.

